To run examples in this directory:

- as standalone simulation:

  > simulavr --device at90s8515 -f fred.elf -W 0x20,- -R 0x22,- -T exit
  
- with tcl interface, but also standalone:

  > ../simulavr.tcl -d at90s8515 -f fred.elf -W 0x20,- -R 0x22,- -T exit
  
- with tcl interface, but as target for gdb:

  > ../simulavr.tcl -d at90s8515 -f fred.elf -W 0x20,- -R 0x22,- -T exit -g
  
To get a .elf for a different cpu (replace AVR_CPU to your cpu!):

  > avr-gcc -g -O2 -mmcu=AVR_CPU -o fred.elf fred.c

